CHxx_QUAD_CHANNEL

Description

> Get or Set the video stream type in the QUAD channel encoder for decoder.

> This URL is used when the CHxx_SOURCE_TYPE=1. In QUAD Encoder, It provides 5 types of video streams to the decoder.

> The mapping of the input argument and the streaming type of the QUAD encoder is listed below.

> Input Argument | Streaming Type | Description
> 0 | QUAD Channel | Four channels are in one single video stream
> 1 | Channel 1 | Channel 1 in QUAD Encoder is in the video stream
> 2 | Channel 2 | Channel 2 in QUAD Encoder is in the video stream
> 3 | Channel 3 | Channel 3 in QUAD Encoder is in the video stream
> 4 | Channel 4 | Channel 4 in QUAD Encoder is in the video stream

> The xx is the channel ID in the decoder started from 01 and ended to 16.

> In EPL decoder device, the xx is fixed to 01.

Input Argument

> 0, 1, 2, 3 or 4

Attribute

- Readable and Writable in EPL Decoders
- Not On-Fly

Return of Message

- Read Operation

> CHxx_QUAD_CHANNEL='0'

- Write Operation

> OK: CHxx_QUAD_CHANNEL='0'
> or
> ERROR: CHxx_QUAD_CHANNEL='0'

Applicability

- EPL Decoder Devices

Status

> Valid

See Also

> CHxx_VIDEO_CONNECT, CHxx_VIDEO_VARFPS, CHxx_VIDEO_STREAM, CHxx_VIDEO_AUDIO, CHxx_VIDEO_CONTROL, CHxx_VIDEO_TCP_IP, CHxx_VIDEO_MULTICAST_IP, CHxx_VIDEO_USERNAME, CHxx_VIDEO_PASSWORD, CHxx_PORT_STREAM, CHxx_PORT_CONTROL, CHxx_PORT_MULTICAST, CHxx_PORT_RTP, CHxx_PORT_HTTP, CHxx_TIME, CHxx_SOURCE_TYPE, CHxx_CHANNEL, SWITCH, VIDEO_VARFPS

Example

- Read Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CHxx_QUAD_CHANNEL
> where xx is from 01~16

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CHxx_QUAD_CHANNEL=0
> where xx is from 01~16

Back to

> HOME, URL CGI