DATE_MANUAL_DATE

Description

> Get or Set Date manual date configuration. The date setting is set as the date locally. The time zone has to be matched the region where the device is deployed.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and the Router's DATE configurations will be returned.

Input Argument

> mmdd0000yyyy
> where
> mm: 01~12 for manual month setting
> dd: 01~31 for manual date setting
> yyyy: ~2035 for manual year setting

Attribute

- Readable and Writable (except all video servers in Multi-Channel Platform)
- On-Fly (except all devices in WPL Platform)

Return of Message

- Read Operation

> DATE_MANUAL_DATE='0101000020004'

- Write Operation

> OK: DATE_MANUAL_DATE='010100002004'
> or
> ERROR: DATE_MANUAL_DATE='010100002004'

Applicability

- WPL Platform : All Encoder Devices
- EPL Platform : All Encoder Devices
- PlatformT : All Encoder Devices
- Multi-Channel Encoder : All Devices

Status

> This URL will be obsolete and replaced by DATE_CONFIG

See Also

> DATE, DATE_TYPE, DATE_SNTP_IP, DATE_SNTP_UPDATE, DATE_MANUAL_TIME, DATE_MANUAL_ZONE, DATE_CONFIG, DAYLIGHT_SAVING_CONFIG

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DATE_MANUAL_DATE
> or
> http://ip:port/cgi-bin/cmd/system?DATE_MANUAL_DATE

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DATE_MANUAL_DATE=010100002004
> or
> http://ip:port/cgi-bin/cmd/system?DATE_MANUAL_DATE=010100002004

Back to

> HOME, SYSTEM CGI