DDNS

Description

> Get the DDNS (Dynmic Domain Name Server) configurations.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, the Router's DNS configurations will be returned.

Input Argument

> None

Attribute

- Read Only

Return of Message

> DDNS_TYPE='1'
> DDNS_HOSTNAME=''
> DDNS_SERVICE='dyndns'
> DDNS_USERNAME=''
> DDNS_PASSWORD=''

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> DDNS_TYPE, DDNS_HOSTNAME, DDNS_SERVICE, DDNS_USERNAME, DDNS_PASSWORD, DDNS_CONFIG, V2_DDNS_CONFIG, WAN_STATUS, V2_WAN_STATUS

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DDNS
> or
> http://ip:port/cgi-bin/cmd/system?DDNS

Back to

> HOME, SYSTEM CGI