DDNS_HOSTNAME

Description

> Get or Set DDNS (Dynamic Domain Name Server) host name configuration. This allows people to access this device through this host name.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and the Router's DDNS configurations will be returned.

Input Argument

> Character strings (< 128 Bytes)

Attribute

- Readable and Writable (except all video servers in Multi-Channel Platform)
- On-Fly (except all devices in WPL Platform)

Return of Message

- Read Operation

> DDNS_HOSTNAME=''

- Write Operation

> OK: DDNS_HOSTNAME='camera1.com'
> or
> ERROR: DDNS_HOSTHANE=''

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : All Devices

Status

> This URL will be obsolete and replaced by DDNS_CONFIG

See Also

> DDNS, DDNS_TYPE, DDNS_SERVICE, DDNS_USERNAME, DDNS_PASSWORD, DDNS_CONFIG, V2_DDNS_CONFIG, WAN_STATUS, V2_WAN_STATUS

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DDNS_HOSTNAME
> or
> http://ip:port/cgi-bin/cmd/system?DDNS_HOSTNAME

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DDNS_HOSTNAME=camera1.com
> or
> http://ip:port/cgi-bin/cmd/system?DDNS_HSTNAME=camera1.com

Back to

> HOME, SYSTEM CGI