OSD_XY

OSD_X, OSD_Y

Description

> Get or Set the beginning position of the OSD information.

> The device could show some information of the encoder and its information on the TV screen. The OSD information will be placed on the upper-left corner on the screen with a specific offset (x,y) in pixels. The URL could get or set this offset of the OSD.

> The range of the input argument are vary from WPL decoders and EPL decoders. Of course, it should make sense to have readable on the TV screen which the video resolution should be concerned.

> The range of OSD offset in WPL decoders is X: 8~96 pixels and Y: 8~96 pixels.

> The range of OSD offset in WPL decoders is X: 1~100 pixels and Y: 1~100 pixels.

Input Argument

> n where is the position in pixel from (0,0) for OSD offset.

Attribute

- Write Only in WPL Decoders
- Readable and Writable in EPL Decoders
- On-Fly

Return of Message

> In WPL Decoder Devices

> - None

> In EPL Decoder Devices

> - Read Operation

> > OSD_X='30'
> > OSD_Y='25'

> - Write Operation

> > OK: OSD_X='30'
> > OK: OSD_Y='25'
> > or
> > ERROR: OSD_X='30'
> > ERROR: OSD_Y='25'

Applicability

- WPL Decoder Devices
- EPL Decoder Devices

Status

> Valid

See Also

> HOST(only available in WPL Decoder Devices), VIDEO_OSD, OSD, OSD_DATE_TIME, OSD_SERVER_IP, OSD_CAMERA_NAME, OSD_LOCAL_IP, OSD_MOTION_DETECT, OSD_STATUS

Example

- Read Operation (Only in EPL Decoder Devices)

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_X
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_Y

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_X=30
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_Y=25

Back to

> HOME, URL CGI