DATE_CONFIG

Description

> Get or Set Date configuration. It allows all Date configurations can be set in one time.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and the Router's DATE configurations will be returned.

Input Argument

> a,b,c,d
> where
> a : DATE type, 1: Manual Date 2: SNTP Synchronization
> b : if a = 1, it is the manual date setting (mmdd0000yyyy), if a = 2, it is the SNTP server address (IPv4 address or host of SNTP server)
> c : if a = 1, it is the manual time setting (mm:ss:hh). if a = 2, it is the SNTP update interval in second
> d : time zone setting

Attribute

- Readable and Writable (except all video servers in Multi-Channel Platform)
- On-Fly

Return of Message

- Read Operation

> DATE_CONFIG='1,010100002004,00:00:00,+00'
> or
> DATE_CONFIG='2,192.168.0.2,86400,+00'

- Write Operation

> OK: DATE_CONFIG='1,010100002004,00:00:00,+00'
> or
> OK: DATE_CONFIG='2,192.168.0.2,86400,+00'
> or
> ERROR: DDNS_TYPE='1,010100002004,00:00:00,+00'
> or
> ERROR: DATE_CONFIG='2,192.168.0.2,86400,+00'

Applicability

- EPL Platform : All Encoder Devices
- PlatformT : All Encoder Devices
- Multi-Channel Encoder : All Devices

Status

> This URL is new command for replacing the URL DATE_TYPE, DATE_SNTP_IP, DATE_SNTP_UPDATE, DATE_MANUAL_DATE, DATE_MANUAL_TIME and DATE_MANUAL_ZONE

See Also

> DATE, DATE_TYPE, DATE_SNTP_IP, DATE_SNTP_UPDATE, DATE_MANUAL_DATE, DATE_MANUAL_TIME, DATE_MANUAL_ZONE, DAYLIGHT_SAVING_CONFIG

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DATE_CONFIG
> or
> http://ip:port/cgi-bin/cmd/system?DATE_CONFIG

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DATE_CONFIG=1,010100002004,00:00:00,+00
> or
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DATE_CONFIG=2,192.168.0.2,86400,+00
> or
> http://ip:port/cgi-bin/cmd/system?DATE_CONFIG=1,010100002004,00:00:00,+00
> or
> http://ip:port/cgi-bin/cmd/system?DATE_CONFIG=2,192.168.0.2,86400,+00

Back to

> HOME, SYSTEM CGI