V2_LOWPASS_FILTER

Description

> Get or Set the encoder's video lowpass function. This function is only available in the encoder in WPL platform and 8CH video server in Multi-Channel Encoder.

Input Argument

> 0 : Disable
> 1 : Enable

Attribute

- Readable and Writable
- Not On-Fly

Return of Message

- Read Operation

> V2_LOWPASS_FILTER='1'

- Write Operation

> OK: V2_LOWPASS_FILTER='1'
> or
> ERROR: V2_LOWPASS_FILTER='1'

Applicability

- WPL Platform : All Encoder Devices
- Multi-Channel Encoder : 8CH video servers

Status

> Valid

See Also

¡@

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_LOWPASS_FILTER
> or
> http://ip:port/cgi-bin/cmd/system?V2_LOWPASS_FILTER

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_LOWPASS_FILTER=1
> or
> http://ip:port/cgi-bin/cmd/system?V2_LOWPASS_FILTER=1

Back to

> HOME, SYSTEM CGI