VIDEO_IRIS

Description

> Get or Set the video IRIS control.

> The IRIS mode and the IRIS level could be accessed by this URL. Please refer the Camera Setup Design Specification for further details.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> n,m
> where
> n: IRIS mode. It could be AUTO or MANUAL
> m: IRIS level. This could be ignored. The mapping of this argument and IRIS level in sensor is listed below.

> Input Argument (m) | IRIS Level in Sensor
> F220 | F22.0
> F190 | F19.0
> F160 | F16.0
> F140 | F14.0
> F110 | F11.0
> F96 | F9.6
> F80 | F8.0
> F68 | F6.8
> F56 | F5.6
> F48 | F4.8
> F40 | F4.0
> F34 | F3.4
> F28 | F2.8
> F24 | F2.4
> F20 | F2.0
> F18 | F.18
> F16 | F1.6
> F14 | F1.4

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_IRIS='AUTO,F20'
> or
> OK: VIDEO_IRIS='AUTO'

- Write Operation

> OK: VIDEO_IRIS='MANUAL,F20'
> or
> ERROR: VIDEO_IRIS='MANUAL,F20'

Applicability

- EPL Platform : All Encoders with sensor MT54G15
- PlatfotmT : All Encoders with sensor MT54G15

Status

> Valid

See Also

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_IRIS
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_IRIS

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_IRIS=AUTO,F20
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_IRIS=AUTO,F20

Back to

> HOME, ENCODER CGI