System CGI Program

Mpeg4 CGI Program

Only root could set the configuration through this MPEG4 CGI. If the logon user is not root, all write commands will be treated as read commands. The CGI is only available in the Encoder Devices. The URL in this CGI will be forwarded to all video servers by router in the Multi-Channel Encoder platform.

NOTE:

> This CGI will be replaced with the Encoder CGI. That will be claimed with the release of device's firmware in the future.

List of URLs

URL | Attribute (R/W, On-Fly)1
WPL Platform | EPL Platfrom | Platform T | Multi-Channel Encoder
Encoder | Encoder | Encoder | Video Server
VIDEO_STATUS | RO,X | RO,X | RO,X | RO,X
VIDEO_CAMERA_NAME | RW,V2 | RW,V | RW,V | RW,V3
VIDEO_BRIGHTNESS | RW,V2 | RW,V | RW,V | RW,V3
VIDEO_CONTRAST | RW,V2 | RW,V | RW,V | RW,V3
VIDEO_SATURATION | RW,V2 | RW,V | RW,V | RW,V3
VIDEO_HUE | RW,V2 | RW,V | RW,V | RW,V3
VIDEO_RESOLUTION | RW,V | RW,V | RW,V | RW,V3
VIDEO_BITRATE | RW,V | RW,V | RW,V | RW,V3
VIDEO_FPS | RW,V | RW,V | RW,V | RW,V3
VIDEO_FPS_NUM | RW,V | RW,V | RW,V | RW,V3
VIDEO_VARIABLE_FPS | WO,V | WO,V | WO,V | WO,V3
DIO_STATUS | RO,X | RO,X | RO,X | RO,X
DIO_OUTPUT | WO,V | WO,V | WO,V | WO,V3
MOTION_STATUS | RO,X | RO,X | RO,X | RO,X
MOTION_ENABLED | RW,V | RW,V | RW,V | RW,V3
MOTION_SETTING | WO,V2 | WO,V | WO,V | WO,V3
MOTION_SENSITIVE | WO,V2 | WO,V | WO,V | WO,V3
SERIAL_SETTING | RW,V | RW,V | RW,V | RW,V3
SERAIL_ASCII | WO,V | WO,V | WO,V | WO,V3
SERIAL_HEX | WO,V | WO,V | WO,V | WO,V3
RTP_MULTICAST_STREAMING | WO,V | WO,V | WO,V | WO,V3

Back to

> HOME

Foot Note

1 | The first part is for Access Mode. It could be RW (Readable and Writeable), RO (Read Only), WO (Write Only) or None (Not Support) The second part is for On-Fly indication. if the change of URL is effective immediately without save and reboot, It could be V (the URL is on-fly). Otherwise, it is X (the URL is not on-fly).
2 | Only be available of 1CH and 2CH Encoder. For Quad Encoders, it is not available.
3 | Return the CHANNEL 1 video server's configuration. If the CHANNEL 1 video server does not connect to router, the error message will be returned