ACTIVEX_URL

Description

> Read the ActiveX URL configuration.

> Currently, the ActiveX URL setting is not used in the device. However, for some applications, the remote host needs to read this setting.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, the Router's ACTIVEX_URL configurations will be returned.

Input Argument

> None

Attribute

- Read Only

Return of Message

- Read Operation

> ACTIVEX_URL=''

Applicability

- WPL Platform : All Encoder Devices
- EPL Platform : All Encoder Devices
- PlatfotmT : All Encoder Devices
- Multi-Channel Encoder : Router Only

Status

> Valid

See Also

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&ACTIVEX_URL
> or
> http://ip:port/cgi-bin/cmd/system?ACTIVEX_URL

Back to

> HOME, SYSTEM CGI