DDNS_CONFIG

Description

> Get or Set DDNS (Dynmic Domain Name Server) configurations.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and Router's DDNS configurations will be returned.

Input Argument

> n : if n = 1 (DDNS is disabled)
> or
> n,a,b,c,d : if n = 2 (DDNS is enabled)
> where
> n : DDNS_TYPE, 1: Disable, 2: Enable
> a : DDNS_HOSTNAME, character string for host name of DDNS (< 128 bytes)
> b : DDNS_SERVICE, name of DDNS service server, dyndns, qdns, ezip, pgpow, dhs, ods, tzo, easydns, justlinux, dyns, hn, zoneedit
> c : DDNS_USERNAME, User Name to logon DDNS service server (< 32 bytes)
> d : DDNS_PASSWORD, User Password to logon DDNS service server (< 32 bytes)

Attribute

- Readable and Writable (except all video servers in Multi-Channel Platform)
- On-Fly

Return of Message

- Read Operation

> DDNS_CONFIG='1,,dyndns,,'

- Write Operation

> OK: DDNS_CONFIG='1'
> or
> OK: DDNS_CONFIG='2,camera1.com,dyndns,root,123'
> or
> ERROR: DNS_CONFIG='1,,dyndns,,'

Applicability

- EPL Platform : Encoder (Version after V3.06.13) and Decoder (Version after V3.01.03)
- PlatformT: Encoder
- Multi-Channel Encoder : All Devices (Router Version after 2.03.03)

Status

> This URL is the new command for replacing the URL DDNS_TYPE, DDNS_HOSTNAME, DDNS_SERVICE, DDNS_USERNAME and DDNS_PASSWORD

See Also

> DDNS, DDNS_TYPE, DDNS_HOSTNAME, DDNS_SERVICE, DDNS_USERNAME, DDNS_PASSWORD, V2_DDNS_CONFIG, WAN_STATUS, V2_WAN_STATUS

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DDNS_CONFIG
> or
> http://ip:port/cgi-bin/cmd/system?DDNS_CONFIG

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DDNS_CONFIG=1 http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DDNS_CONFIG=2,camera1.com,dyndns,root,123
> or
> http://ip:port/cgi-bin/cmd/system?DDNS_CONFIG=1,,dyndns,,
> http://ip:port/cgi-bin/cmd/system?DDNS_CONFIG=2,camera1.com,dyndns,root,123

Back to

> HOME, SYSTEM CGI