AUDIO_MIC_BOOST

Description

> Set the AudioIn Sensitivity configuration. Check the device specification is needed before use this command. Only two-way audio device supports this URL.

> There are two levels for this volume control. They are 0dB and 20dB. Here is the mapping table of input argument and these four volume levels.

> Value of Input argument | Volume Level
> 0 | 0dB
> 1 | 20dB

Input Argument

> 0 or 1

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> AUDIO_MIC_BOOST='1'

- Write Operation

> OK: AUDIO_MIC_BOOST='1'
> or
> ERROR: AUDIO_MIC_BOOST='1'

Applicability

- EPL Decoder Devices

Status

> Valid

See Also

> AUDIO_SET_VOL

Example

- Read Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&AUDIO_MIC_BOOST

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&AUDIO_MIC_BOOST=1

Back to

> HOME, URL CGI