MOTION_ENABLED

Description

> Get or set Motion Enabled configuration. The parameter is in the hexadecimal format.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's MOTION_ENABLED configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> None

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: MOTION_ENABLED='0x00'

- Write Operation

> OK: MOTION_ENABLED='0x00'
> or
> ERROR: MOTION_ENABLED='0x00'

Applicability

- WPL Platform : All Encoders
- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : All Video Servers

Status

> Valid

See Also

- In mpeg4 CGI

> MOTION_STATUS, MOTION_SETTING, MOTION_SENSITIVITY

- In encoder CGI

> MOTION_CONFIG, MOTION_CONFIG_GET, MOTION_SENSITIVITY, MOTION_TIMER, MOTION_OBJ

Example

- Read Operation

> http://ip:port/cgi-bin/CGI?USER=Admin&PWD=123456&MOTION_ENABLED
> or
> http://ip:port/cgi-bin/cmd/CGI?MOTION_ENABLED

> where CGI could be mpeg4 or encoder

- Write Operation

> http://ip:port/cgi-bin/CGI?USER=Admin&PWD=123456&MOTION_ENABLED=0x00
> or
> http://ip:port/cgi-bin/cmd/CGI?MOTION_ENABLED=0x00

> where CGI could be mpeg4 or encoder

Back to

> HOME, MPEG4 CGI, ENCODER CGI