PORT_SEARCH1_2

PORT_SEARCH_1, PORT_SEARCH_2

Description

> Get or Set device search server port numbers. We provide some utilities like IPUtility to find all our devices in the intranet through these UDP search ports.

> When write, the port number will be checked if it was used from other applications

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and the Router's search server port number will be returned.

Input Argument

> UDP port number, 1~65535

Attribute

- Readable and Writable (except all video servers in Multi-Channel Encoder)
- On-Fly (except all devices in WPL Platform)

Return of Message

- Read Operation

> PORT_SEARCH_1='6005'

> PORT_SEARCH_2='6006'

- Write Operation

> OK: PORT_SEARCH_1='6005'
> OK: PORT_SEARCH_2='6006'
> or
> ERROR: PORT_SEARCH_1='6005'
> ERROR: PORT_SEARCH_2='6006'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : All Devices

Status

> This URL will be obsolete and replaced by PORT_SEARCH

See Also

> PORT, PORT_HTTP, PORT_SEARCH, PORT_REGISTER, PORT_CONTROL, PORT_VIDEO, PORT_MULTICAST, V2_PORT_RTSP, V2_PORT_RTP_MULTI_VIDEO, V2_PORT_RTP_MULTI_AUDIO

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&PORT_SEARCH_1
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&PORT_SEARCH_2
> or
> http://ip:port/cgi-bin/cmd/system?PORT_SEARCH_1
> http://ip:port/cgi-bin/cmd/system?PORT_SEARCH_2

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&PORT_SEARCH_1=6005
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&PORT_SEARCH_2=6006
> or
> http://ip:port/cgi-bin/cmd/system?PORT_SEARCH_1=6005
> http://ip:port/cgi-bin/cmd/system?PORT_SEARCH_2=6006

Back to

> HOME, SYSTEM CGI