VIDEO_SHUTTER_SPEED

Description

> Get or Set the manual shutter speed.

> This URL will not take effect if only of the VIDEO_SHUTTER_MODE is MANUAL and the shutter speed setting has to match the flickless configuration, refer to VIDEO_FLICKLESS. Please refer the Camera Setup Design Specification for further details.

> The available

> The error message will be returned if the encoder does not support this URL.

Input Argument

> 30, 60, 120, 25, 50, 100, 250, 500, 1000, 2000, 5000, 10000
> where the shutter speed is the 1/(input argument). For example, the shutter speed is 1/30 sec when the input argument is 30.

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_SHUTTER_SPEED='1/60'

- Write Operation

> OK: VIDEO_SHUTTER_SPEED='1/60'
> or
> ERROR: VIDEO_SHUTTER_SPEED='1/60'

Applicability

- EPL Platform : All Encoders with sensor MT9V135 or MT9M131
- PlatfotmT : All Encoders with sensor MT9M131

Status

> Valid

See Also

> VIDEO_WB_MODE, VIDEO_WB_GAIN, VIDEO_EXPOSURE_MODE, VIDEO_EXPOSURE_GAIN, VIDEO_AGC_GAIN, VIDEO_SUHTTER_MODE, VIDEO_MAX_SHUTTER, VIDEO_FLICKLESS

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_SHUTTER_SPEED
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_SHUTTER_SPEED

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_SHUTTER_SPEED=1/60
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_SHUTTER_SPEED=1/60

Back to

> HOME, ENCODER CGI