MOTION_SENSITIVITY

MOTION_SENSITIVE

Description

> Set the motion sensitivity to the specific motion region.

> The higher motion sensitivity, higher probability of motion detection trigger.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the error message will be returned.

Input Argument

> n,sen
> where
> n is the motion region started from 1
> sen is the sensitivity of the motion region and the range is 0~100.

Attribute

- Write Only
- On-Fly

Return of Message

- Write Operation

> OK: MOTION_SENSITIVE='1,50'
> or
> ERROR: MOTION_SENSITIVE='1,50'

Applicability

- WPL Platform : All 1CH and 2CH Encoders
- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : All Video Servers

Status

> Valid

See Also

- In mpeg4 CGI

> MOTION_STATUS, MOTION_ENABLED, MOTION_SETTING

- In encoder CGI

> MOTION_ENABLED, MOTION_CONFIG, MOTION_CONFIG_GET, MOTION_TIMER, MOTION_OBJ

Example

- Write Operation

> http://ip:port/cgi-bin/CGI?USER=Admin&PWD=123456&MOTION_SENSITIVE=1,50
> or
> http://ip:port/cgi-bin/cmd/CGI? MOTION_SENSITIVE=1,50

> where CGI could be mpeg4 or encoder

Back to

> HOME, MPEG4 CGI, ENCODER CGI