V2_FAILOVER

Description

> Get or Set the failover function.

> In WPL Encoder Platform, the LAN port could be act as the backup port which be able to take over the traffic form WAN when the WAN connection is broken. Once the WAN connection is recovered, the LAN will hand over the traffic to WAN. This is only available in all WPL encoders.

> Once the failover is enabled, the LAN port will not be functional until the WAN port connection is broken.

Input Argument

> 0 : Disable
> 1 : Enable

Attribute

- Readable and Writable
- Not On-Fly

Return of Message

- Read Operation

> V2_FAILOVER='0'

- Write Operation

> OK: V2_FAILOVER='1'
> or
> ERROR: V2_FAILOVER='1'

Applicability

- WPL Platform : All Encoder Devices
- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : 8CH video server

Status

> Valid

See Also

> ¡@

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_FAILOVER
> or
> http://ip:port/cgi-bin/cmd/system?V2_FAILOVER

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_FAILOVER=0
> or
> http://ip:port/cgi-bin/cmd/system?V2_FAILOVER=0

Back to

> HOME, SYSTEM CGI