ADDR

Description

> Get or Set the address setting for PTZ command parser.

> For IP Camera, this URL is useless. For a Video Server, this URL could get or set the analog PTZ camera address. Refer to PTZ Design Specification for further details.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's ADDR configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> 0xnn where nn is the hexadecimal value from 00~FF.

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: ADDR='0x01'

- Write Operation

> OK: ADDR='0x01'
> or
> ERROR: ADDR='0x01'

Applicability

- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : 4CH and 16CH Video Servers

Status

> Valid

See Also

> PTZ_VENDOR, ZOOM, ZOOM_POSITION, FOCUS, FOCUS_POSITION, MOVE, MOVE_LIMIT, MOVE_LIMIT_GET, MOVE_MAX_SPEED_GET, POSITION, POSITION_GET

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&ADDR
> or
> http://ip:port/cgi-bin/cmd/encoder?ADDR

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&ADDR=0x01
> or
> http://ip:port/cgi-bin/cmd/encoder? ADDR=0x01

Back to

> HOME, ENCODER CGI