OSD_ENABLED

Description

> Control of the OSD (On Screen Display) function.

> The input argument of this command is hexadecimal value. It controls how many types of information could be shown on the OSD. Here is the map of the input hexadecimal value and the information type on OSD.

> Bit value in the input argument | Type of information on OSD
> Bit 0 | Video (Channel) Title Name
> Bit 1 | Video Loss Trigger
> Bit 2 | Motion Detection Trigger
> Bit 3 | Date and Time
> Bit 4 | DIO status

> The bit value is 1, the corresponding device information will be shown on the OSD. And the bit value is 0, the corresponding device information will not be shown on the OSD.

Input Argument

> 0xnn
> where
> nn : in hexadecimal and decoded in bit-wise for type of device information on OSD.

> Note that the value in higher bit (bit 5~7) will not effect the OSD display function and there is no error message returned if the higher bit (but 5~7) is not zero.

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OSD_ENABLED='0x0f'

- Write Operation

> OSD_ENABLED='0x0f'
> or
> ERROR: OSD_ENABLED Value Failed (if the setting is lager than 0xff)

Applicability

- WPL Platform : QUAD Encoder Only

Status

> Valid

See Also

> MOTION_ENABLED, TITLE_NAME

Example

- Read Operation

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&OSD_ENABLED

- Write Operation

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&OSD_ENABLED=0x0f

Back to

> HOME, QUAD CGI