VOL_AUDIOOUT

Description

> Set the AudioOut volume configuration. Check the device specification is needed before use this command. Only audio device supports this URL.

> There are four levels for this volume control. They are mute, small, middle and large. Here is the mapping table of input argument and these four volume levels.

> Value of Input argument | Volume Level
> 0 | mute
> 1 | small
> 2 | middle
> 3 | large

Input Argument

> 0, 1, 2 or 3

Attribute

- Write Only
- Not On-Fly

Return of Message

> None

Applicability

- WPL Decoder Devices

Status

> Valid

See Also

> HOST(only available in WPL Decoder Devices), VOL_AUDIOIN

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&VOL_AUDIOOUT=1

Back to

> HOME, URL CGI