BAUDRATE

Description

> Set the baud rate of serial port.

> There is a serial port on the device for the RS232/RS485/RS422 port. The external device could be accessed or controlled through this port. For example, when the RS485 port in Analog PTZ camera connects to the Video Server's serial port, user could control this Analog PTZ camera through the Video Sever by Joystick connected to Decoder's RS232/RS485/RS422 port.

> Note that, there is no any hardware and software flow control mechanism implemented in this serial port. For example, the RS485 port in Joystick connects to the Decoder's serial port.

Input Argument

> baud rate. It could be 2400, 4800, 9600, 19200, 38400, 57600, 115200

Attribute

- Write Only
- Not On-Fly

Return of Message

> None

Applicability

- WPL Decoder Devices

Status

> Valid

See Also

> HOST(only available in WPL Decoder Devices), UARTSETTING

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&BAUDRATE=9600

Back to

> HOME, URL CGI