SPEED_WAN

Description

> Get or Set link speed and duplex mode of WAN port.

> In Multi-Channel device, this URL will be read-only command if the CHANNEL=n was set before this URL. Then, the return message will be WAN_SPEED='0' always.

Input Argument

> 0: Auto Negotiation
> 1: Force to 100Mbps and Full Duplex Mode
> 2: Force to 100Mbps and Half Duplex Mode
> 3: Force to 10Mbps and Full Duplex Mode
> 4: Force to 10Mbps and Half Duplex Mode

Attribute

- Readable and Writable (except the video server in Multi-Channel Device)
- On-Fly (except all WPL Platform devices)

Return of Message

- Read Operation

> WAN_SPEED='0'

- Write Operation

> OK: WAN_SPEED='0'
> or
> ERROR: WAN_SPEED='0'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> SPEED_LAN

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&SPEED_WAN
> or
> http://ip:port/cgi-bin/cmd/system?SPEED_WAN

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&SPEED_WAN=n
> or
> http://ip:port/cgi-bin/cmd/system?SPEED_WAN=n

Back to

> HOME, SYSTEM CGI