VIDEO_WB_GAIN

VIDEO_AGC_GAIN

Description

> Get or Set the ACG Target Gain.

> The video Exposure Gain is only configurable if only of the VIDEO_EXPOSURE_MODE is AUTO. Please refer the Camera Setup Design Specification for further details.

> Note that the ACG Target Gain affects the video exposure much. The higher AGC Target Gain, the more sensitivity of light condition. It might be very easy to cause the over exposure when it has better light condition.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> 1~100 for Gain value

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_AGC_GAIN='55'

- Write Operation

> OK: VIDEO_AGC_GAIN='55'
> or
> ERROR: VIDEO_AGC_GAIN='55'

Applicability

- EPL Platform : All Encoders with sensor MT9V135 or MT9M131
- PlatfotmT : All Encoders with sensor MT9M131

Status

> Valid

See Also

> VIDEO_WB_MODE, VIDEO_WB_GAIN, VIDEO_EXPOSURE_MODE, VIDEO_EXPOSURE_GAIN, VIDEO_SHUTTER_MODE, VIDEO_SUHTTER_SPEED,VIDEO_MAX_SHUTTER, VIDEO_FLICKLESS

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_AGC_GAIN
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_AGC_GAIN

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_AGC_GAIN=55
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_AGC_GAIN=55

Back to

> HOME, ENCODER CGI