WAN

Description

> Get the WAN port configuration. If the WAN Type is Dynamic, the networking address (IP, Netmask and Gateway) in the return message is not the runtime setting.

> In WPL decoder, the DNS and DDNS configurations will be replied in this URL.

> In EPL decoder, this URL is same as the WAN in the SYSTEM CGI but only Type1 URL command is supported.

> Therefore, the WAN URL in WPL decoders is only addressed in this page.

Input Argument

> None

Attribute

- Read Only
- Not On-Fly

Return of Message

>     WAN_TYPE='1'
>     WAN_IP='10.0.0.1'
>     WAN_NETMASK='255.255.255.0'
>     WAN_GATEWAY='10.0.0.254'
>     WAN_PPPOE_USERNAME=''
>     WAN_PPPOE_PASSWORD=''
>     DNS_PRIMARY=''
>     DNS_SECONDARY=''
>     DDNS_TYPE='1'
>     DDNS_SERVICE='dyndns'
>     DDNS_HOSTNAME='ACTi'
>     DDNS_USERNAME=''
>     DDNS_PASSWORD=''

Applicability

- WPL Decoder Devices
- EPL Decoder Devices (refer to WAN in the SYSTEM CGI)

Status

> Valid

See Also

> WAN_TYPE, WAN_IP, WAN_NETMASK, WAN_GATEWAY, WAN_PPPOE_USERNAME, WAN_PPPOE_PASSWORD

Example

> http://ip:port/cgi-bin/url-cgi?USER=Admin&PWD=123456&WAN

Back to

> HOME, URL CGI, SYSTEM CGI