RS232_TEST

Description

> Loopback the Serial Port on the firmware side. This will echo the input data from the RXD in Serial Port to TXD in Serial Port by firmware.

> This is for test only and should be used internally.

Input Argument

> None

Attribute

- Write Only
- On-Fly

Return of Message

> None

Applicability

- EPL Encoder Devices

Status

> Valid

See Also

> NETWORKACCESS_STOP, SET_FRAME_Q_LEN, AUDIO_LOOP_BACK

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&RS232_TEST

Back to

> HOME, URL CGI