RTP_MULTICAST_STREAMING

Description

> Set the RTP streaming type.

> This URL make effect if only if the V2_STREAMING_METHOD is "RTP Over UDP and Multicast". This inform the encoder to be the RTP streaming server with unicast or multicast streaming method.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the error message will be returned.

Input Argument

> PLAY : the multicast RTP streaming method is applied
> PAUSE: the unicast RTP streaming method is applied

Attribute

- Write Only
- On-Fly

Return of Message

- Write Operation

> OK: RTP_MULTICAST_STREAMING='OK'

> or

> ERROR: RTP_MULTICAST_STREAMING='OK'

Applicability

- WPL Platform : All Encoders
- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : All Video Servers

Status

> Valid

See Also

> V2_STREAMING_METHOD

Example

- Write Operation

> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&SRTP_MULTICAST_STREAMING=OK
> or
> http://ip:port/cgi-bin/cmd/mpeg4? RTP_MULTICAST_STREAMING=OK

Back to

> HOME, MPEG4 CGI