MOTION_OBJ

Description

> Set the motion object size to the specific motion region.

> The motion region was divided into several microblocks (16x16 pixel in a motion block). Every microblock has it own calculation of motion detection. This object gives an threshold of the number of motion triggered microblocks in the motion region. For example, there are 200 microblocks in a motion region and the object is set to 10. The motion detection will be triggered when the number of motion triggered microblocks is higher than 20 in this region.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the error message will be returned.

Input Argument

> n,obj
> where
> n is the motion region started from 1
> obj is the motion timer in unit of second and the range is 1~300.

Attribute

- Write Only
- On-Fly

Return of Message

- Write Operation

> OK: MOTION_OBJ='1,70'
> or
> ERROR: MOTION_OBJ='1,70'

Applicability

- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : 4CH and 16CH Video Servers

Status

> Valid

See Also

- In mpeg4 CGI

> MOTION_STATUS, MOTION_ENABLED, MOTION_SETTING, MOTION_SENSITIVITY

- In encoder CGI

> MOTION_ENABLED, MOTION_SENSITIVITY, MOTION_CONFIG, MOTION_CONFIG_GET, MOTION_TIMER

Example

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&MOTION_OBJ=1,70
> or
> http://ip:port/cgi-bin/cmd/encoder? MOTION_OBJ=1,70

Back to

> HOME, MPEG4 CGI, ENCODER_CGI