LANGUAGE

Description

> Get or Set Language configuration.

> Currently, there are several language sets available in the device. The mapping of the language index and language set is listed below. Because the language set is added from time to time and might be vary from device to device. It needs to check the specification of the device to know how many and which language sets are available for a device.

> Mapping table of language index and language set

> Language Index | Language Set | Character Set
> 0 | English | UTF-8
> 1 | Traditional Chinese | BIG5
> 2 | Simplified Chinese | BG2312
> 3 | Japanese | EUC-JP
> 4 | Spanish | ISO-8859-1
> 5 | Italian | ISO-8859-1
> 6 | German | ISO-8859-1
> 7 | Portuguese | ISO-8859-1
> 8note1 | Czech | ISO-8859-1
> 9 | French | ISO-8859-1
> 10 | Finnish | ISO-8859-1
> 11 | Hungarian | ISO-8859-2
> 12 | Dnish | ISO-8859-1

> note 1 : Not available now

Input Argument

> 0~Max Language index (= 9).

Attribute

- Write Only in WPL Decoders
- Readable and Writable in EPL Decoders
- On-Fly

Return of Message

- None in WPL Decoders
- Same as the LANGUAGE in SYSTEM CGI

Applicability

- WPL Decoder Devices
- EPL Decoder Devices

Status

> Valid

See Also

> HOST(only available in WPL Decoder Devices),

Example

- Read Operation (Only in EPL Decoder Devices)

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&LANGUAGE

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&LANGUAGE=0

Back to

> HOME, URL CGI, SYSTEM CGI