DDNS_SERVICE

Description

> Get or Set DDNS (Dynamic Domain Name Server) service server configuration. Currently, it provides the 12 predefined DDNS service servers to subscribe the DDNS services. There is no guarantee if these DDNS service servers are available from time to time.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and the Router's DDNS configurations will be returned.

Input Argument

> dyndns: members.dyndns.org
> qdns : members.3322.org
> ezip: www.ez-ip.net
> pgpow: www.penguinpowered.com
> dhs: members.dhs.org
> ods: update.ods.org
> tzo: cgi.tzo.com
> easydns:members.easydns.com
> justlinux: www.justlinux.com
> dyns: www.dyns.com
> hn: www.hn.org
> zoneedit: www.zoneedit.com

Attribute

- Readable and Writable (except all video servers in Multi-Channel Platform)
- On-Fly (except all devices in WPL Platform)

Return of Message

- Read Operation

> DDNS_SERVICE='dyndns'

- Write Operation

> OK: DDNS_SERVICE='dyndns'
> or
> ERROR: DDNS_SERVICE='dyndns'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : All Devices

Status

> This URL will be obsolete and replaced by DDNS_CONFIG

See Also

> DDNS, DDNS_TYPE, DDNS_HOSTNAME, DDNS_USERNAME, DDNS_PASSWORD, DDNS_CONFIG, V2_DDNS_CONFIG, WAN_STATUS, V2_WAN_STATUS

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DDNS_SERVICE
> or
> http://ip:port/cgi-bin/cmd/system?DDNS_SERVICE

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DDNS_SERVICE=dyndns
> or
> http://ip:port/cgi-bin/cmd/system?DDNS_SERVICE=dyndns

Back to

> HOME, SYSTEM CGI