VIDEO_TV

Description

> Get or Set Analog TV setting (NTSC or PAL) for Video Out.

> The range of input argument of this URL is vary from WPL decoders and EPL decoders.

> In WPL decoder, the "NTSC" and "PAL" strings are used as the input argument of this URL.

> In EPL decoder, the "0" and "1" are used as the input argument of this URL. The "0" means the PAL and "1" means the NTSC.

Input Argument

> NTSC or PAL in WPL decoder
> or
> 0 or 1 in EPL decoder

Attribute

- Write Only in WPL Decoders
- Readable and Writable in EPL Decoders
- On-Fly (except EPL Decoders)

Return of Message

> In WPL Decoder Devices

> - None

> In EPL Decoder Devices

> - Read Operation

> > VIDEO_TV='1'

> - Write Operation

> > OK: VIDEO_TV='1'
> > or
> > ERROR: VIDEO_TV='1'

Applicability

- WPL Decoder Devices
- EPL Decoder Devices

Status

> Valid

See Also

> HOST(only available in WPL Decoder Devices)

Example

- Read Operation (Only in EPL Decoder Devices)

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&VIDEO_TV

- Write Operation

> In WPL Decoder Devices

> > http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&VIDEO_TV=NTSC

> In EPL Decoder Devices

> > http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&VIDEO_TV=1

Back to

> HOME, URL CGI