OSD_DATE_TYPE

Description

> Get or Set the format of the displaying date on the TV screen.

> There are three formats of the date on OSD. Here is the mapping table of the input argument of this URL and format of the date.

> Value of Input Argument | Format of Date | Description
> 0 | YYMMDD | YY: Year, MM : month, DD Date
> 1 | MMDDYY
> 2 | DDMMYY

Input Argument

> 0,1 or 2

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OSD_DATE_FORMAT='1'

- Write Operation

> OK: OSD_DATE_FORMAT='1'
> or
> ERROR: OSD_DATE_FORMAT='1'
> ¡@

Applicability

- EPL Decoder Devices

Status

> Valid

See Also

> OSD_X, OSD_Y, OSD_DATE_TIME, OSD_SERVER_IP, OSD_CAMERA_NAME, OSD_LOCAL_IP, OSD_MOTION_DETECT, OSD_STATUS

Example

- Read Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_DATE_FORMAT

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_DATE_FORMAT=1

Back to

> HOME, URL CGI