VIDEO_STATUS

Description

> Get the video configuration.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the CHANNEL 1 video server's VIDEO_STATUS configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> None

Attribute

- Read Only

Return of Message

>     VIDEO_BRIGHTNESS='25'
>     VIDEO_CONTRAST='15'
>     VIDEO_SATURATION='67'
>     VIDEO_HUE='50'
>     VIDEO_RESOLUTION='N1280x1024'
>     VIDEO_BITRATE='3M'
>     VIDEO_FPS='MODE1'
>     VIDEO_FPS_NUM='8'
>     VIDEO_CAMERA_NAME='Camera-1'

Applicability

- WPL Platform : All Encoders
- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : All Video Servers

Status

> Valid

See Also

> VIDEO_BRIGHTNESS, VIDEO_CONTRAST, VIDEO_SATURATION, VIDEO_HUE, VIDEO_RESOLUTION, VIDEO_BITRATE, VIDEO_FPS, VIDEO_FPS_NUM, VIDEO_CAMERA_NAME

Example

> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_STATUS
> or
> http://ip:port/cgi-bin/cmd/mpeg4?VIDEO_STATUS

Back to

> HOME, MPEG4 CGI