LAN_ADDRESS

LAN_IP, LAN_NETMASK

Description

> Set IP or Netmask address of LAN port.

Input Argument

> IPv4 Addressing (xxx.xxx.xxx.xxx)

Attribute

- Write Only
- Not On-Fly

Return of Message

> None

Applicability

- WPL Decoder Devices

Status

> Valid

See Also

> HOST(only available in WPL Decoder Devices), LAN_HOSTNAME

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&LAN_IP=192.168.1.254
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&LAN_NETMASK=255.255.255.0

Back to

> HOME, URL CGI