MOVE

Description

> Perform the pan and tilt functions.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the error message will be returned.

> MOVE Command | Description
> UP,SpeedTilt | Move camera up with a specific speed.
> DOWN,SpeedTilt | Move camera down with a specific speed.
> LEFT,SpeedPan | Move camera left with a specific speed.
> RIGHT,SpeedPan | Move camera right with a specific speed.
> UPLEFT,SpeedPan,SpeedTilt | Move camera up and left with specific speeds.
> UPRIGHT,SpeedPan,SpeedTilt | Move camera up and right with specific speeds.
> DOWNLEFT,SpeedPan,SpeedTilt | Move camera down and left with specific speeds.
> DOWNRIGHT,SpeedPan,SpeedTilt | Move camera down and right with specific speeds.
> STOP | Stop the Pan and Tilt action.
> HOME | Move camera to home position
> RESET | Reset camera position to factory default position

> For PTZ IP Camera, the MOVE=STOP should be sent after another MOVE command except HOME and RESET commands had been sent.

> If the URL does not bring the SpeedTilt and SpeedPan, the current pan and tilt speeds will be used. In UPLEFT, UPRIGHT, DOWNLEFT and DOWNRIGHT commands, the SpeedPan and SpeedTilt have to be set or not be set together.

> The SpeedPan and SpeedTilt are in hexadecimal and started from 0x1 (slowest) to 0x5 (fastest)

> There are five levels in SpeedPan and SpeedTilt. The PTZ camera might have more levels of them. In case, the linear scaling algorithm will be used for that.

Input Argument

> Refer to above command table

Attribute

- Write Only
- On-Fly

Return of Message

- Write Operation

> OK: echo of command
> or
> ERROR: echo of command

Applicability

- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : 4CH and 16CH Video Servers

Status

> Valid

See Also

> ADDR, PTZ_VENDOR, ZOOM, ZOOM_POSITION, FOCUS_POSITION, MOVE_LIMIT, MOVE_LIMIT_GET, MOVE_MAX_SPEED_GET, POSITION, POSITION_GET

Example

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&MOVE=UPLEFT,0x1,0x3
> or
> http://ip:port/cgi-bin/cmd/encoder?MOVE=UPLEFT,0x1,0x3

Back to

> HOME, ENCODER CGI