CHxx_CHANNEL

Description

> Get or Set the the Mutli-Channel Encoder's channel ID to decoder.

> This URL is used when the CHxx_SOURCE_TYPE=2. In Multi-Channel Encoder, the maximum channel could be 16. Please refer to the Multi-Channel encoder specification for further details. The Channel ID in Multi-Channel encoder is started from 1.

> The xx is the channel ID in the decoder started from 01 and ended to 16.

> In EPL decoder device, the xx is fixed to 01.

Input Argument

> 1~16

Attribute

- Readable and Writable in EPL Decoders
- Not On-Fly

Return of Message

- Read Operation

> CHxx_CHANNEL='0'

- Write Operation

> OK: CHxx_CHANNEL='0'
> or
> ERROR: CHxx_CHANNEL='0'

Applicability

- EPL Decoder Devices

Status

> Valid

See Also

> CHxx_VIDEO_CONNECT, CHxx_VIDEO_VARFPS, CHxx_VIDEO_STREAM, CHxx_VIDEO_AUDIO, CHxx_VIDEO_CONTROL, CHxx_VIDEO_TCP_IP, CHxx_VIDEO_MULTICAST_IP, CHxx_VIDEO_USERNAME, CHxx_VIDEO_PASSWORD, CHxx_PORT_STREAM, CHxx_PORT_CONTROL, CHxx_PORT_MULTICAST, CHxx_PORT_RTP, CHxx_PORT_HTTP, CHxx_TIME, CHxx_SOURCE_TYPE, CHxx_QUAD_CHANNEL, SWITCH, VIDEO_VARFPS

Example

- Read Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CHxx_CHANNEL
> where xx is from 01~16

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CHxx_CHANNEL=0
> where xx is from 01~16

Back to

> HOME, URL CGI