MOTION_TIMER

Description

> Set the motion timer to the specific motion region.

> The motion timer means the time interval in second started from a motion trigger (in control session) does not have motion trigger again. In other words, the remote host will not receive two successive motion triggers in control session during the motion time interval. Note that the motion trigger in video B2 data will not be affected by this timer.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the error message will be returned.

Input Argument

> n,timer
> where
> n is the motion region started from 1
> timer is the motion timer in unit of second and the range is 1~300.

Attribute

- Write Only
- On-Fly

Return of Message

- Write Operation

> OK: MOTION_TIMER='1,10'
> or
> ERROR: MOTION_TIMER='1,10'

Applicability

- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : 4CH and 16CH Video Servers

Status

> Valid

See Also

- In mpeg4 CGI

> MOTION_STATUS, MOTION_ENABLED, MOTION_SETTING, MOTION_SENSITIVITY

- In encoder CGI

> MOTION_ENABLED, MOTION_SENSITIVITY, MOTION_CONFIG, MOTION_CONFIG_GET, MOTION_OBJ

Example

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&MOTION_TIMER=1,10
> or
> http://ip:port/cgi-bin/cmd/encoder? MOTION_TIMER=1,10

Back to

> HOME, MPEG4 CGI, ENCODER_CGI