VIDEO_CAMERA_NAME

Description

> Get or set the name of the device. This name could be used to identify the camera or video server from devices.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's VIDEO_CAMERA_NAME configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> Character string (<32 bytes)

Attribute

- Readable and Writable
- On-Fly

Return of Message

-     Read Operation

> OK: VIDEO_CAMERA_NAME='Camera-1'

- Write Operation

> OK: VIDEO_CAMERA_NAME='Camera-1'
> or
> ERROR: VIDEO_CAMERA_NAME='Camera-1'

Applicability

- WPL Platform : All 1CH and 2CH Encoders
- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : All Video Servers

Status

> Valid

See Also

¡@

Example

- Read Operation

> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_CAMERA_NAME
> or
> http://ip:port/cgi-bin/cmd/mpeg4?VIDEO_CAMERA_NAME

- Write Operation

> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_CAMERA_NAME=Camera-1
> or
> http://ip:port/cgi-bin/cmd/mpeg4?VIDEO_CAMERA_NAME=Camera-1

Back to

> HOME, MPEG4 CGI