DECODER CGI Program

This CGI provides the URL command to access the Decoder devices.

Only root could set the configuration through this CGI. If the logon user is not root, all write commands will be treated as read commands.

NOTE:

> The URL CGI which is old fashion CGI used for Decoder Devices. It will be divided into two parts of URLs. One will be migrated to the SYSTEM CGI and the other one will be moved and modified in this CGI.

> This CGI is available only for the firmware version after B1X-A2-B2.05.06 in WPL Decoders.

> This CGI is available only for the firmware version after B1D-220-V3.02.00 in EPL Decoders.

List of URLs

> URL | Attribute (R/W, On-Fly)1
> WPL Decoder | EPL Decoder | PlatformT Decoder
> OSD | RO,X | RO,X | RO,X
> OSD_FORMAT | RW,V | RW,V | RW,V
> OSD_POSITION | RW,V | RW,V | RW,V
> OSD_POSITION_RANGE | RO,V | RO,V | RO,V
> OSD_DATE_FORMAT | RW,V | RW,V | RW,V
> CHANNEL_CONFIG | RW,V | RW,V | RW,V
> CHANNEL_VARIABLE_FPS | RW,V | RW,V | RW,V
> CHANNEL_TIME | RW,V | None | RW,V
> CHANNEL_INFO | RO,X | RO,X | RO,X
> CHANNEL_SWITCH | WO,V | None | WO,V

Back to

> HOME

Foot Note

1 | Access Mode. It could be RW (Readable and Writeable), RO (Read Only), WO (Write Only) or None (not supported)