FW_UPG_STATUS

Description

> Show the status of the firmware upgrade status to the remote host.

> The mapping of the return code and the status of firmware upgrade is listed below.

> Return Code | Status of firmware upgrade
> 0 | The firmware upgrade has not been issued
> 1 | The firmware upgrade is in progress
> 100 | The firmware upgrade was completed
> 110 | The firmware version is incorrect
> 111 | The firmware image was corrupted (firmware/MD5 file upload error or MD5 checksum error)
> 112 | The firmware Type is in correct (AC/NB was mismatched)

Input Argument

> None

Attribute

- Read Only
- Not On-Fly

Return of Message

> FW_UPG_STATUS='n'
> where n could be 0, 1, 100, 110, 111, 112

Applicability

- WIS Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Encoder Devices
- Multi-Channel Encoder : Router Only

Status

> Valid

See Also

> UPDATE CGI

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&FW_UPG_STATUS
> or
> http://ip:port/cgi-bin/cmd/system?FW_UPG_STATUS

Back to

> HOME, SYSTEM CGI