SPEED_LAN

Description

> Get or Set link speed and duplex mode of LAN port.

> Consider the compatibility with ISV, this URL is set to read-only command for the device without LAN port like all EPL Platform, PlatformT and Multi-Channel devices. Then, the return message of this URL is LAN_SPEED='0' always.

Input Argument

> 0: Auto Negotiation
> 1: Force to 100Mbps and Full Duplex Mode
> 2: Force to 100Mbps and Half Duplex Mode
> 3: Force to 10Mbps and Full Duplex Mode
> 4: Force to 10Mbps and Half Duplex Mode

Attribute

- Readable and Writable for all WPL Platform Devices
- Read Only for all EPL Platform, PlatformT and Multi-Channel Devices. The return message is LAN_SPEED='0' always.
- Not On-Fly

Return of Message

- Read Operation

> LAN_SPEED='0'

- Write Operation

> OK: LAN_SPEED='0'
> or
> ERROR: LAN_SPEED='0'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatformT : All Devices

Status

> Valid

See Also

> SPEED_WAN

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&SPEED_LAN
> or
> http://ip:port/cgi-bin/cmd/system?SPEED_LAN

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&SPEED_LAN=n
> or
> http://ip:port/cgi-bin/cmd/system?SPEED_LAN=n

Back to

> HOME, SYSTEM CGI