WAN_TYPE

Description

> Get or Set WAN connection type. Three types, Dynamic, Static and PPPoE, are supported.

> In Dynamic connection type, the device will try to get the IP/Netmask/Gateway/DNS settings from a DHCP server.

> In Static connection type, the device will use WAN_IP, WAN_NETMASK and WAN_GATEWAY to configure its WAN port.

> In PPPoE connection type, the device will try to establish the PPP connection. The WAN_PPPOE_USERNAME and WAN_PPPOE_PASSWORD will be used for authentication.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL will be treated as read-only command and the Router's WAN connection type will be returned.

Input Argument

> 1: Dynamic
> 2: Static
> 3: PPPoE

Attribute

- Readable and Writable
- Not On-Fly

Return of Message

- Read Operation

> WAN_TYPE='1'

- Write Operation

> OK: WAN_TYPE='1'
> or
> ERROR: WAN_TYPE='1'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> WAN, WAN_STATUS, V2_WAN_STATUS, WAN_IP, WAN_NETMASK, WAN_GATEWAY, WAN_PPPOE_USERNAME, WAN_PPPOE_PASSWORD

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&WAN_TYPE
> or
> http://ip:port/cgi-bin/cmd/system?WAN_TYPE

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&WAN_TYPE=1
> or
> http://ip:port/cgi-bin/cmd/system?WAN_TYPE=1

Back to

> HOME, SYSTEM CGI