AUDIO_OUT_VOLUME

Description

> Get or Set the AudioOut volume configuration. Check the device specification is needed before use this command. Only two-way audio device supports this URL.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's AUDIO_OUT_VOLUME configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> 0~100

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> AUDIO_OUT_VOLUME='50'

- Write Operation

> OK: AUDIO_OUT_VOLUME='50'
> or
> ERROR: AUDIO_OUT_VOLUME='50'

Applicability

- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> AUDIO_OUT_LEVEL

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&AUDIO_OUT_VOLUME
> or
> http://ip:port/cgi-bin/cmd/system?AUDIO_OUT_VOLUME

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&AUDIO_OUT_VOLUME=50
> or
> http://ip:port/cgi-bin/cmd/system?AUDIO_OUT_VOLUME=50

Back to

> HOME, SYSTEM CGI