VIDEO_BLC_MODE

Description

> Get or Set the VIDEO Back Light Compensation Mode configuration.

> Please refer the Camera Setup Design Specification for further details.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> 0: Turn off BLC function, 1: Turn on BLC function

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_BLC_MODE='1'

- Write Operation

> OK: VIDEO_BLC_MODE='1'
> or
> ERROR: VIDEO_BLC_MODE='1'

Applicability

- EPL Platform : All Encoders with sensor MT54G15
- PlatfotmT : All Encoders with sensor MT54G15

Status

> Valid

See Also

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_BLC_MODE
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_BLC_MODE

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_BLC_MODE=1
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_BLC_MODE=1

Back to

> HOME, ENCODER CGI