DATE_TYPE

Description

> Get or Set Date type configuration. Some devices have RTC which the date and time will keep working even the power was unplugged. Based on the Date type, the device will set the date and time properly. Then, the device's date and time information will be carried by video streams.

> If the Date type is SNTP synchronization, the device date and time might be started by Manual date and time settings if it fails of connecting to NTP server and there is no RTC.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and the Router's DATE configurations will be returned.

Input Argument

> 1: Manual Date Type
> 2: SNTP Synchronization

Attribute

- Readable and Writable (except all video servers in Multi-Channel Platform)
- On-Fly (except all encoders in WPL Platform)

Return of Message

- Read Operation

> DATE_TYPE='2'

- Write Operation

> OK: DATE_TYPE='2'
> or
> ERROR: DATE_TYPE='2'

Applicability

- WPL Platform : All encoder Devices
- EPL Platform : All encoder Devices
- PlatformT : All encoder Devices
- Multi-Channel Encoder : All Devices

Status

> This URL will be obsolete and replaced by DATE_CONFIG

See Also

> DATE, DATE_SNTP_IP, DATE_SNTP_UPDATE, DATE_MANUAL_DATE, DATE_MANUAL_TIME, DATE_MANUAL_ZONE, DATE_CONFIG, DAYLIGHT_SAVING_CONFIG

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DATE_TYPE
> or
> http://ip:port/cgi-bin/cmd/system?DATE_TYPE

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DATE_TYPE=2
> or
> http://ip:port/cgi-bin/cmd/system?DATE_TYPE=2

Back to

> HOME, SYSTEM CGI