MOVE_LIMIT

Description

> Set or Clear the maximum movement limitation in pan and tilt directions.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the error message will be returned.

> MOVE Command | Description
> SET,Direction,PostionPan,PositionTilt | Set the maximum movement limitation of camera
> CLR,Direction | Reset the maximum movement limitation to the factory default setting

> The Direction could be UPRIGHT or DOWNLEFT.

> The PositionPan and PositionTilt are in hexadeciaml started from 0x0 to 0xFFFF. The PTZ camera might not have such wide range of these positions. However, the device will NOT validate them before parser and handle this URL. Please refer to the device specification to have correct pan and tilt position ranges.

> In CLR command, the device will try to match the Direction. If it matches, remove the movement limitation. The MOVE_LIMIT_GET returns current movement limitation setting after this CLR command.

Input Argument

> Refer to above command table

Attribute

- Write Only
- On-Fly

Return of Message

- Write Operation

> OK: echo of command
> or
> ERROR: echo of command

Applicability

- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : 4CH and 16CH Video Servers

Status

> Valid

See Also

> ADDR, PTZ_VENDOR, ZOOM, ZOOM_POSITION, FOCUS_POSITION, MOVE, MOVE_LIMIT_GET, MOVE_MAX_SPEED_GET, POSITION, POSITION_GET

Example

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&MOVE_LIMIT=SET,UPRIGHT,0x5643,0x3743
> or
> http://ip:port/cgi-bin/cmd/encoder?MOVE_LIMIT=SET,UPRIGHT,0x5643,0x3743
> or
> http://ip:port/cgi-bin/cmd/encoder?USER=Admin&PWD=123456&MOVE_LIMIT=CLR,UPRIGHT
> or
> http://ip:port/cgi-bin/cmd/encoder?MOVE_LIMIT=CLR,UPRIGHT

Back to

> HOME, ENCODER CGI