V2_MULTICAST_IF

Description

> Get or Set the networking interface (LAN or WAN port) for sending/receiving multicast packets.

> In WPL Platform, there are two networking interface, LAN and WAN port,. By default, the multicast path is on LAN port. It needs to switch the multicast path to WAN port if your networking connection is on the WAN port.

> In EPL, PlatformT and Multi-Channel devices, there is only one networking port (WAN). It does not need to set this configuration. However, for back compatible consideration, this command needs to be supported in Read Only way and return 1 (WAN) always.

Input Argument

> 1 : WAN Port
> 2 : LAN Port

Attribute

- Readable and Writable
- Not On-Fly

Return of Message

- Read Operation

> V2_MULTICAST_IF='1'

- Write Operation

> OK: V2_MULTICAST_IF='1'
> or
> ERROR: V2_MULTICAST_IF='1'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> PORT_MULTICAST, V2_PORT_RTP_MULTI_VIDEO, V2_PORT_RTP_MULTI_AUDIO, VIDEO_MULTICAST_TTL, V2_MULTICAST_IP, IGMP_ENABLED

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_MULTICAST_IF
> or
> http://ip:port/cgi-bin/cmd/system?V2_MULTICAST_IF

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_MULTICAST_IF=1
> or
> http://ip:port/cgi-bin/cmd/system?V2_MULTICAST_IF=1

Back to

> HOME, SYSTEM CGI