PORT

Description

> Get the device's networking port number configurations. The return message of this command depends on the type of devices. In Encoder devices. the HTTP, search, register, control, video and multicast port numbers will be returned. In Decoder devices, the HTTP and search port numbers will be returned.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the CHANNLE 1 video server's PORT configurations will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> None

Attribute

- Read Only

Return of Message

> Form Encoder Devices:

> > PORT_HTTP='80'
> > PORT_SEARCH_1='6005'
> > PORT_SEARCH_2='6006'
> > PORT_REGISTER='6000'
> > PORT_CONTROL='6001'
> > PORT_VIDEO='6002'
> > PORT_MULTICAST='5000'

> Form Decoder Devices:

> > PORT_HTTP='80'
> > PORT_SEARCH_1='6005'
> > PORT_SEARCH_2='6006'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> PORT_HTTP, PORT_SEARCH_1, PORT_SEARCH_2, PORT_SEARCH, PORT_REGISTER, PORT_CONTROL, PORT_VIDEO, PORT_MULTICAST, V2_PORT_RTSP, V2_PORT_RTP_MULTI_VIDEO, V2_PORT_RTP_MULTI_AUDIO

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&PORT
> or
> http://ip:port/cgi-bin/cmd/system?PORT

Back to

> HOME, SYSTEM CGI