DATE

Description

> Get the Date configurations.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, the Router's Date configurations will be returned.

Input Argument

> None

Attribute

- Read Only

Return of Message

> DATE_TYPE='2'
> DATE_SNTP_IP='192.168.0.2'
> DATE_SNTP_UPDATE='86400'
> DATE_MANUAL_DATE='010100002004'
> DATE_MANUAL_TIME='00:00:00'
> DATE_MANUAL_ZONE='+00'

Applicability

- WPL Platform : All Encoder Devices
- EPL Platform : All Encoder Devices
- PlatfotmT : All Encoder Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> DATE_TYPE, DATE_SNTP_IP, DATE_SNTP_UPDATE, DATE_MANUAL_DATE, DATE_MANUAL_TIME, DATE_MANUAL_ZONE, DATE_CONFIG, DAYLIGHT_SAVING_CONFIG

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DATE
> or
> http://ip:port/cgi-bin/cmd/system?DATE

Back to

> HOME, SYSTEM CGI