VIDEO_SENSEUP_LEVEL

Description

> Get or Set the Sensor's Sense UP level configuration.

> This URL set the lighting level to sensor to determine when the sensor should issue or terminate the Sense Up. Please refer the Camera Setup Design Specification for further details.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> 0~255

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_SENSEUP_LEVEL='50'

- Write Operation

> OK: VIDEO_SENSEUP_LEVEL='AUTO'
> or
> ERROR: VIDEO_SENSEUP_LEVEL='AUTO'

Applicability

- EPL Platform : All Encoders with sensor MT54G15
- PlatfotmT : All Encoders with sensor MT54G15

Status

> Valid

See Also

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_SENSEUP_LEVEL
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_SENSEUP_LEVEL

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_SENSEUP_LEVEL=50
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_SENSEUP_LEVEL=50

Back to

> HOME, ENCODER CGI