PORT_HTTP

Description

> Get or Set device's http server port number. When write, the port number will be checked if it was used from other applications.

> In EPL decoder, this URL is same as the PORT_HTTP in the SYSTEM CGI but only Type1 URL command is supported.

> Therefore, the PORT_HTTP URL in WPL decoders is only be addressed in this page.

Input Argument

> TCP port number, 1~65535

Attribute

- Write Only
- Not On-Fly

Return of Message

> None

Applicability

- WPL Decoder Devices
- EPL Decoder Devices (refer to PORT_HTTP in the SYSTEM CGI)

Status

> Valid

See Also

> PORT, PORT_HOST_SEARCH_1, PORT_HOST_SEARCH_2

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&PORT_HTTP=80

Back to

> HOME, URL CGI, SYSTEM CGI